Factory Details:
  Rank                     none (0)
  Long-name                NDI track data source
  Klass                    Source
  Description              Sends Track From Device
  Author                   NDI

Plugin Details:
  Name                     ndielems
  Description              NDI plugins
  Filename                 C:\gstreamer\1.0\x86_64\lib\gstreamer-1.0\ndielems.dll
  Version                  1.8.1
  License                  LGPL
  Source module            gstreamer
  Source release date      2019-06-14
  Binary package           GStreamer
  Origin URL               http://gstreamer.net/

GObject
 +----GInitiallyUnowned
       +----GstObject
             +----GstElement
                   +----GstBin
                         +----GstTrackBin

Implemented Interfaces:
  GstChildProxy

Pad Templates:
  SRC template: 'src'
    Availability: Always
    Capabilities:
      video/x-raw
                 format: { (string)RGBx, (string)RGB, (string)BGR, (string)BGRx, (string)xRGB, (string)xBGR, (string)RGBA, (string)BGRA, (string)ARGB, (string)ABGR, (string)I420, (string)YV12, (string)AYUV, (string)YUY2, (string)UYVY, (string)v308, (string)v210, (string)v216, (string)Y41B, (string)Y42B, (string)Y444, (string)YVYU, (string)NV12, (string)NV21, (string)UYVP, (string)RGB16, (string)BGR16, (string)RGB15, (string)BGR15, (string)UYVP, (string)A420, (string)YUV9, (string)YVU9, (string)IYU1, (string)ARGB64, (string)AYUV64, (string)r210, (string)I420_10LE, (string)I420_10BE, (string)GRAY8, (string)GRAY16_BE, (string)GRAY16_LE }
                  width: [ 1, 2147483647 ]
                 height: [ 1, 2147483647 ]
              framerate: [ 0/1, 2147483647/1 ]

Element has no clocking capabilities.
Element has no URI handling capabilities.

Pads:
  SRC: 'src'

Element Properties:
  name                : The name of the object
                        flags: readable, writable
                        String. Default: "trackbin0"
  parent              : The parent of the object
                        flags: readable, writable
                        Object of type "GstObject"
  async-handling      : The bin will handle Asynchronous state changes
                        flags: readable, writable
                        Boolean. Default: false
  message-forward     : Forwards all children messages
                        flags: readable, writable
                        Boolean. Default: false
  connect-to          : Name of NDI device to connect to
                        flags: readable, writable
                        String. Default: "P9-00311.local"
  rtsp-port           : RTSP port for the video connection
                        flags: readable, writable
                        String. Default: "554"
  tool-location       : Directory location of the tool files that will be loaded
                        flags: readable, writable
                        String. Default: "C:/Tool Definition Files/"
  tool-file           : Name of a tool rom file to load
                        flags: readable, writable
                        String. Default: "8700339.rom"

Children:
  KLVTimeStampBin
  H264VideoBin
  VegaRTSPSource
  NDITrackOverlay
  NDItrackSource
  TrackQueue
